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DEVELOPMENT PERMIT - MCUI/29/2009
Citation

This Development Permit shall be cited as No: MCUI/29/2009.

Application Details

	Application Type:
	Material Change of Use 

	Application Description:
	Public Worship (Extension)


Land

This Development Permit applies to the following land:

	Street Address:
	4915-4923 Mount Lindesay Highway, SOUTH MACLEAN  QLD  4280

	Real Property Description:
	Lot 423 WD 3792


Development Permit

· This Development Permit is granted in accordance with the Conditions of Development

· This development permit will take effect, in accordance with 3.5.19 of the Integrated Planning Act
· The Currency Period of this development permit will lapse in accordance with 3.5.21 of the Integrated Planning Act
Conditions of Development

The conditions of Development for this Development Permit are as follows:

1.
premises
1.1
Comply with the provisions of Council's Local Laws, Planning Scheme Policies, Planning Scheme and Planning Scheme Codes to the extent they have not been varied by this approval.

2.
TIMING OF COMPLIANCE WITH CONDITIONS

2.1
Comply with all conditions prior to commencement of the use, unless otherwise stated within an individual condition. 

3.
PLAN OF DEVELOPMENT
3.1
Undertake the development generally in accordance with the plans listed in the following table, except as amended below or otherwise altered by this approval:

	Drawing No.
	Title
	Prepared by
	Received by Council

	BA01 Iss. A
	Temple Renovation Site Plan
	D&S Design & Drafting
	30 June 2009

	BA05 Iss. D
	Temple Renovation Floor Plan - Proposed
	D&S Design & Drafting
	30 June 2009

	BA06 Iss. B
	Temple Renovation Roof Plan - Proposed
	D&S Design & Drafting
	30 June 2009

	BA07 Iss. A
	Temple Renovation Elevations - Proposed
	D&S Design & Drafting
	30 June 2009

	BA08 Iss. A
	Temple Renovation Sections - Proposed
	D&S Design & Drafting
	30 June 2009

	BA09 Iss. B
	Toilet Block Renovation Existing & Proposed
	D&S Design & Drafting
	30 June 2009

	BA10 Iss. A
	Vali Pillayar Renovation Existing & Proposed
	D&S Design & Drafting
	30 June 2009

	BA12 Iss. A
	Caretakers Residence Proposed
	D&S Design & Drafting
	30 June 2009

	BA13 Iss. A
	Caretakers Residence Proposed (Elevations)
	D&S Design & Drafting
	30 June 2009

	BA14 Iss. A
	Education Hall Proposed Plan
	D&S Design & Drafting
	30 June 2009

	BA15 Iss. A
	Education Hall Proposed Elevations
	D&S Design & Drafting
	30 June 2009

	BA16 Iss. A
	Annathana Area Proposed
	D&S Design & Drafting
	30 June 2009


4.
contributions

4.1
Pay a contribution to Council towards Water Supply Infrastructure in accordance with the Planning Scheme applicable at the time of payment, based on 0.74 ET. Payment must be made at the time of application for the Compliance Certificate for any part of the development under the Plumbing and Drainage Act 2002, or prior to the commencement of use, whichever occurs first.
Advisory Note: Charges are subject to indexation which will be applied at the time of payment. 

5.
Planning

5.1
Conduct the development in accordance with the following restrictions:

5.1.1
Education Hall:
5.1.1.1
Restrict use of the hall to Sundays. Do not conduct educational activities onsite during weekdays without obtaining a Development Permit for an 'Educational Establishment'.
5.1.1.2
Do not exceed a student capacity of approximately ten (10) students.
5.1.2
Festivals:
5.1.2.1
Hours of operation of festivals are restricted to 9AM - 9PM, and for no more than approximately 3 hours duration within that period. 

5.1.2.2
Limit noise levels to those in accordance with the requirements of the Environmental Protection (Noise) Policy 2008. In the event Council receives a validated noise related complaint, immediately reduce noise levels to the relevant levels in accordance with EPP (Noise) 2008 requirements.
5.1.3
Child Care:

5.1.3.1
Restrict child care usage to primarily be conducted on Sundays in association with the 'Public Worship' land use.

5.1.3.2
Do not exceed a capacity of seven (7) children on weekdays without obtaining a Development Permit for a 'Child Care Facility'.

5.1.4
Caretakers Residence:
5.1.4.1
Restrict use to one family unit and associated guests.
Advisory Note: The plans for the Caretakers Dwelling detail attached self contained rooms with individual entrances. Be advised that renting these rooms individually may trigger the definition of 'Motel' under the Beaudesert Shire Planning Scheme and require a Permit.
6.
ACCESS AND PARKING

6.1
Construct access to the site from Henderson Street generally in accordance with the approved plans. Incorporate the construction of a minimum 5.5 m wide road with a two-way reinforced concrete driveway crossover, in accordance with Council standard drawing number 50416. 

Advisory Note: A Council Technical officer must inspect and approve the driveway prior to bitumen sealing.
6.2
Upgrade Henderson Street from Mt. Lindesay Highway up to the proposed entry/exit point of the development to a two coat bitumen sealed road, with a minimum 6m width.
6.3
Design and construct all access and internal layout for the turning movements of a 'Heavy Rigid Vehicle'.
6.4
Construct the car park area of sealed bitumen.
6.5
Design the car parking for the development in compliance with the Beaudesert Shire Planning Scheme 2007 and Australian Standard 2890.1.
7.
STORMWATER

7.1
Provide stormwater drainage in accordance with the provisions of the Beaudesert Shire Planning Scheme 2007, the Queensland Urban Drainage Manual, and the 'Stormwater Management Plan', written by Lenehan Consulting, and received by Council on 4 December 2009. Design and construct the stormwater drainage to address the following:

7.1.1
Underground stormwater drain lines and/or overland flow drainage path within easements (where necessary) incorporating all external catchments; 

7.1.2
Underground drain lines to connect the site to Council’s stormwater drainage system if such system is available;

7.1.3
No 'worsening' of peak flows currently exiting the site;

7.1.4
All site drainage;

Advisory Note: Existing dam onsite is considered a legal point of discharge provided 'no worsening' of stormwater occurs at the property boundary. 

8.
GENERAL
8.1
Pay the full cost of any alteration necessary to electricity, telephone, water mains, sewer mains, stormwater drainage systems or easements and/or other public utility installations resulting from the development or from road and drainage works required in connection with the development. Install all services underground.

8.2
Do not commence works which will ultimately revert to Council, or on adjacent roads or drainage schemes, until Council has been advised in writing of the name of the responsible contractor and that the contractor has received from Council a notice of appointment of principal contractor under the provisions of the Workplace Health and Safety Act.

9.
plumbing & drainage

9.1
Replace the existing septic system with an appropriate HSTP system, in accordance with a Plumbing and Drainage approval from Council. 

9.2
Apply for and obtain a Plumbing and Drainage approval for the additions to, disconnection, alteration or relocation of, existing sanitary plumbing and drainage and on-site sewerage facility and effluent disposal area.

10.
Lighting

10.1
Ensure any onsite illumination does not exceed an illumination level of 8 lux, measured from 1.5 metres outside the site.

11.
Landscaping

11.1
Submit and have approved by Council a landscape plan and documentation, prepared by a Corporate Member of the Australian Institute of Landscape Architects, (or other suitably qualified and experienced professional deemed suitable on demonstration of project experience and document skills to Council), as part of a development application for Operational Works - Landscaping, prior to Building Works approval.  Design the landscape plan and documentation generally in accordance with the approved site plan prepared by Design & Drafting, drawing number BA01 Issue A dated June 2009. Prepare plan in accordance with the provisions of Council's Landscaping Code, Planning Scheme Policies and include the following:

· Landscape areas at natural ground level except where it is proposed to import soil with suitable retaining works;

· No hardstand surfacing including car parking areas located within the drip line of any retained vegetation;

· Provision of a 5 metre wide landscape buffer along the site boundary adjoining all rural residential areas, incorporating existing vegetation where possible;

· A densely planted landscape buffer a minimum 5 metres wide along the Mt Lindsay highway frontage.  Landscaping to create a visual screen of no less than 3 metres in height.  New trees to be planted at a minimum 4 metre centres, with shrubs located throughout, to achieve a dense screening layer, and groundcovers concentrated to the boundaries of the buffer area,  incorporating existing vegetation where possible;

· Location of all existing vegetation to be retained and indicate the proposed protection methods during construction;

· Provision of information on basic drainage indicating the direction of flow into drainage swales/paths or gully pits to ensure no ponding/pooling of water;  

· Provide a planting plan and include a diverse selection of native trees, shrubs and groundcovers to reinforce the local character of the area;

· All plants to be drought tolerant;

· Turf to be drought resistant and shade tolerant;

· Maintenance in accordance with the BSC design and construction manual.

12.1
Erosion and sediment control

12.1
Implement appropriate erosion and sediment control measures on site prior to the commencement of works taking place, to ensure that erosion is minimised and water quality standards are not compromised during any works on site.

12.2
Restore the site and any adjoining affected lands where sediment deposition has occurred as a consequence of operational works activity associated with the development. Complete such restoration in a reasonable time as determined by the Manager - Development Assessment.

13.
Construction Control

13.1
Do not use reticulated water for construction purposes while Level 4 or higher water restrictions are in place within the City of Logan. Only recycled water obtained from Council's sewerage treatment plant at Loganholme or any similar approved source can be used for construction purposes. 
13.2
Do not commence on works which will ultimately revert to Council or on adjacent roads or drainage schemes until Council has been advised in writing, of the name of the responsible contractor and that the contractor has received from Council a notice of appointment of principal contractor under the provisions of the Workplace Health and Safety Act.

This is the end of conditions for Development Permit Number MCUI/29/2009.
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